. Windows 95
1. run "setup" to install VIA PCI IRQ Routing Miniport Driver.

. Windows 98
Before install Win98.
1. Enable "OnChip USB" in BIOS Chipset Features setup menu.
2. Enable "Assign IRQ for USB" in PNP/PCP Configuration Setup menu.
After Installing Win98
1. run "setup" to install VIA PCI IRQ Routing Miniport Driver.

History:
V1.3A: to pass Norton Win doctor's test.
V1.3: fix VT596 routing error in Win95
