------------------------------------------------------------------------------------------------
                                 Readme file	

此目录下的各驱动适应于WINDOWS95操作系统,WINDOWS98系统可不用安装.

------------------------------------------------------------------------------------------------
Copyright (c) Trend Corp., Winbond Inc., HighPoint Inc, Intel Corp., Via Inc., Award Corp, Adobe Inc. .

------------------------------------------------------------------------------------------------






$$ Via PCI Bridge Driver -- The setup program supports to register VIA chipset's functions in 
   Windows 95 and Windows 98. The functions include USB and ACPI.

Installation Procedure:
1. Run setup and select "install VIA Chipset Functions' Registry", then it will 
automatically install this program.

You can see that it displays "VIA Power Management Controller" and 
"VIA PCI to USB Universal Host Controller".

NOTE: If user want to upgrade Windows 95 to Windows 95 OSR 2.1 (4.00.950 B),
it's necessary to remove USB from other device.

------------------------------------------------------------------------------------------------
********* Notes : 1. Via PCI Bridge Driver is only for Win95/Win98 
                  2. You can go to the below directory to get more information in the CD.
                     \DRIVERV\PCIBridge\Readme.txt
------------------------------------------------------------------------------------------------





$$ Via VxD Driver -- This driver should be installed on a system with the VIA AGP chipset, 
   VT82C597 or later, and others' chipsets will not be supported. The VIA VxD Driver is only 
   supported by Windows 95 OSR 2.1 (4.00.950 B) or later version.

For Win95 users,you will need to
1. Get "USBSUPP.EXE" from Microsoft, which includes the USB supplement
   and a new memory manager (VMM32.VxD) needed for the AGP DIME (Direct
   Memory Execute) feature. 
2. Get DirectX 5.0 from Microsoft. DirectX 5.0 is the first DirectX version
   that supports AGP's DIME. 
3. Get AGP Master (i.e., AGP VGA) Driver from VGA Supplier.
4. Get "VIAGART.VXD", a virtual device manager which usually will be
   installed in the following installation procedure of the Windows 95 card
   driver.

For WinNT users, you will have to wait until WinNT 5.0 is released.

------------------------------------------------------------------------------------------------
********* Notes : 1. Via VxD Driver is only for Win95/Win98 
                  2. You can go to the below directory to get more information in the CD.
                     \DRIVERV\AGPVxD\Readme.txt
------------------------------------------------------------------------------------------------





$$ Via Mini-Port Driver -- Windows 98 IRQ rounting table don't match MVP3/ VP3  chipset, 
   that will cause win98 cannot be installed if the board is based on MVP3 / VP3 chipset. 
   the driver can modify the IRQ rounting table to install Win98 well.

------------------------------------------------------------------------------------------------
********* Notes :1. Via Mini Port Driver is only for Win98 
                 2. The Via Mini Port driver is purposed for MVP3/VP3 chipset, 
                    Via Apollo Pro chipset don't need the driver and can install Win98 well.
------------------------------------------------------------------------------------------------




