
  			   =-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=
	                   Solo-1 PCI AudioDrive for Windows 95/98
        	           =-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=



=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=
Installation Instructions for Windows 95
=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=

1. Windows 95 should automatically detect Solo-1 PCI AudioDrive.
2. When the "New Hardware Found" dialog box prompts for a driver, select
   "Driver from disk provided by hardware manufacturer" and insert the
   CD into the CDROM.
3. Select the correct path d:\audio\w95 (assume that d is CD-ROM) 
   and click "OK".
4. Click "OK". The driver files will then be copied.
5. When prompted, click "Yes" to restart the computer.




=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=
Installation Instructions for Windows 98
=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=

1. Windows 98 should automatically detect the Solo-1 PCI AudioDrive.
2. When the "Add New Hardware" dialog box prompts for a driver, select
   "Display a list of all the drivers in a specific location,so you can select
    the driver you want." and click on "Next".
3. Select the " Sound,video and game controllers" and click on "Next".
4. Click on  "Have Disk".
5. Insert the CD.
6. Select the correct path d:\audio\w95 (assume that d is CD-ROM) 
   and click "OK".
7. Click "OK". The driver files will then be copied.
8. When prompted, click "Yes" to restart the computer.