ESS Sound Device for Windows 95 Driver

Installaion

  1. Start Windows 95
  2. Remove the "PCI Multimedia Audio Device" item in the "Device Manager".
     (Control Panel-->System-->Device Manager-->Other Devices)
  3. Reboot the system
  4. Windows 95 will auto detect the sound device as "PCI Multimedia Audio
     Devie" and prompt you for the correct path of the driver.
  5. Insert the disk and enter the path of the driver (such as "D:\AUDIO\WIN95\",
     which "D:" is your CD-ROM). Also, you may use the "BROWSE" button to locate
     the correct path.
  6. The audio driver will be displayed (such as "ES1946 PCI AudioDrive").
  7. Select "Finish" and follow the instructions to complete the installation. 
  