*********************************************************** 
** ENU *************************************************** 
*********************************************************** 
*                                                           
*  Intel(R) Chipset Software Installation Utility
*  Installation Readme                                                           
*
************************************************************
************************************************************


************************************************************
*  CONTENTS OF THIS DOCUMENT
************************************************************
This document contains the following sections:

1.  Overview
2.  System Requirements
3.  Contents of the Distribution Package
4.  List of Available Command Line Flag Options 
5.  Contents of the Extracted Files
6.  Installing the Software in Interactive Mode
7.  Installing the Software in Silent Mode
8.  Installing the INF Files Prior to OS Installation
    8A. Installing the Windows* 2000 INF Files Prior
        to OS Installation
    8B. Installing the Windows* 98/Windows 98 SE/Windows* Me 
        INF Files Prior to OS Installation
    8C. Installing the Windows* 95 INF Files Prior to OS
        Installation
9.  Installing the INF Files After OS Installation
    9A. Installing the Windows* 2000 INF Files after
        OS Installation
    9B. Installing the Windows* 98/Windows* 98 SE/
        Windows* Me/Windows* 95 INF Files after OS
        Installation
10. Verifying Installation of the Software
11. Identifying the Software Version Number
12. Troubleshooting


************************************************************
* 1.  OVERVIEW
************************************************************
The Intel(R) Chipset Software Installation Utility installs
to the target system the Windows* INF files that outline to 
the operating system how the chipset components will be 
configured.  This is needed for the proper functioning of
the following features:

   - Core PCI and ISAPNP Services
   - AGP Support
   - IDE/ATA33/ATA66 Storage Support
   - USB Support
   - Identification of Intel Chipset Components in 
     Device Manager

This software can be installed in three modes: Interactive,
Silent and Unattended Preload.  The Interactive Mode 
requires user input during installation; the Silent Mode and
Unattended Preload do not.  

Additionally, this software offers a set of command line
flag options that enable extended installation 
functionality. The command line flags are not case-
sensitive.  See Section 4 for detailed descriptions of these 
flags.

Important Note:
The Intel(R) Chipset Software Installation Utility is 
distributed in two formats -- self extracting .EXE files
(INFINST_xxx.EXE) or compressed .ZIP files 
(INFINST_xxx.ZIP). Depending on which distribution format is 
being executed, the command-line syntax may differ. See 
Section 4 for more details. 


************************************************************
* 2.  SYSTEM REQUIREMENTS 
************************************************************
1.  The software included with this distribution package is 
    designed to operate with the following chipset 
    configurations:

       Intel(R) 440BX AGPset                            
       Intel(R) 440DX AGPset                            
       Intel(R) 440EX AGPset
       Intel(R) 440GX AGPset
       Intel(R) 440LX AGPset
       Intel(R) 440ZX AGPset
       Intel(R) 440MX Chipset
       Intel(R) 430TX PCIset
       Intel(R) 810  Chipset      
       Intel(R) 810E Chipset
       Intel(R) 810E2 Chipset      
       Intel(R) 815 Chipset       
       Intel(R) 815E Chipset
       Intel(R) 815EM Chipset
       Intel(R) 815EP Chipset
       Intel(R) 815P Chipset       
       Intel(R) 820 Chipset       
       Intel(R) 820E Chipset
       Intel(R) 840 Chipset       
       Intel(R) 850 Chipset
       Intel(R) 860 Chipset
       Intel(R) 830M Chipset     
       Intel(R) 845 Chipset
     
              
2.  One of the following operating systems must be 
    fully installed and running on the system
    before installing this software:

    Windows* 95      4.00.950   (Original Release)
    Windows* 95      4.00.950a  (OSR1)
    Windows* 95      4.00.950b  (OSR2 without USB 
                                Supplement)
    Windows* 95      4.00.950b  (OSR2.1 with USB 
                                Supplement)
    Windows* 95      4.00.950c  (OSR2.5 with or 
                                without USB Supplement)
    Windows* 98      4.10.1998  (Original Release)
    Windows* 98 SE   4.10.2222  (Original Release)
    Windows* Me      4.90.3000  (Original Release)
    Windows* 2000    5.00.2195  (Original Release)
    Windows* XP	     5.10.2465  (Beta 2)
    

    To verify which operating system has been installed onto 
    the target system, follow the steps below:

    a.  Click on Start.
    b.  Select Settings.
    c.  Select Control Panel.
    d.  Double-click on the System icon.
    e.  Click on the General system properties tab.
    f.  Verify, which OS has been installed by reading
        the System information.
                              
3.  It is recommended that the software be installed on 
    systems with at least 32MB of system memory when using 
    Windows* 9x and Windows* Me. Windows* 2000 requires at 
    least 64MB of system memory.


4.  It is recommended that there be sufficient hard disk 
    space in the <TEMP> directory (typically 
    C:\WINDOWS\TEMP) on the system, in order to install this 
    software.

5.  Check the System Requirements.  The operating system 
    must be fully installed and running on the system before
    running this software.

6.  Close any running applications.  Otherwise, you may
    experience difficulties.

7.  It is recommended that the Intel(R) Chipset Software 
    Installation utility be installed onto the target system 
    prior to the installation of other drivers.


Please check with your system provider to determine which 
operating system and Intel chipset are used in your system.


************************************************************
* 3.  CONTENTS OF THE DISTRIBUTION PACKAGE
************************************************************
The Intel(R) Chipset Software Installation Utility package 
contains the following items:

    File(s)       
    -------
    INFINST_xxx.EXE -or- INFINST_xxx.ZIP
    README.TXT, RELNOTES.HTM

RELNOTES.HTM is available in English only.


   *** NOTE:  Only the files that reference the currently 
              detected devices are copied to the system.
	        For a complete list of the INF files, refer to 
              the RELNOTES.HTM file.

              If the -A option is exercised, the files are
              not copied to the <Windows>\INF directory.
              See Section 4 for more information.  

                                       
************************************************************
* 4.  LIST OF AVAILABLE COMMAND LINE FLAG OPTIONS
************************************************************
The Intel(R) Chipset Software Installation Utility supports  
several command line flags for various installation options. 
All command line flags and parameters must be separated by a 
space, except for the language code after the '-L' flag.

Due to the different distribution formats available for the
Intel(R) Chipset Software Installation Utility, the command
line flag syntax may vary:

1. Self-Extracting .EXE Distribution:
      When installing this software using the .EXE 
      distribution, an extra '-A' must be appended to the 
      INFINST_xxx.EXE program call (i.e. INFINST_ENU.EXE -A) 
      in order to successfully pass command line parameters.  
      The extra '-A' flag for the self-extracting .EXE 
      package is DIFFERENT from the '-A' command line flag 
      option described below.  

      Example: To extract INF files using the '-A' flag 
               described below, the installation program 
               should be invoked as follows:  
          
               INFINST_ENU.EXE -A -A (optional -P)

2. Compressed .ZIP Distribution:
      When installing this software using the .ZIP 
      distribution, there is no need to append any extra 
      flags to the SETUP.EXE program call in order to pass 
      command line flags.

      Example: To extract INF files using the '-A' flag 
               described below, the installation program 
               should be invoked as follows:  
                        
               SETUP.EXE -A (optional -P)

Below is a list of all the available command line flags that
may be used with the program call.  Note that the '-L' and 
the '-S' flags MUST be specified at the end of the command 
line flag list.

Flag            Description
----            -----------
-?              Help flag.  Displays the list of available 
                command line flags.  This parameter works in 
                the Interactive mode only.  

-A              Extracts the INF files and README.TXT to 
                either "C:\Program Files\Intel\InfInst" or 
                the <Installation Path> directory specified 
                using the '-P' flag. The software will 
                NOT install these INF files to the system.  
                This flag can be combined only with the '-P' 
                flag option. All other options will be 
                ignored if the '-A' flag is specified. 
                This parameter works in either Silent mode 
                or Interactive mode.

-B              Automatically reboots the system after 
                installation. This flag is ignored if '-A' 
                flag is specified. This parameter works in 
                either Silent mode or Interactive mode.

-L<LangCode>    Forces the InstallShield user interface to 
                display the specified language during setup.  
                Note that there should be NO spaces between 
                '-L' and the 4-digit language code (see 
                below). This flag and the '-S' flag must be 
                placed at the end of the command line flag 
                list. This parameter works in Interactive 
                mode only.

-OVER AUD	Overrides the default behavior of the 
                installer with respect to update of the 
                Audio controller device.

-P <Installation Path>   
                Specifies the HDD location to which the INF 
                program files are copied.  If this flag is 
                not specified at the command line, the 
                <Installation Path> directory is by default 
                assumed to be:
                
                   C:\Program Files\Intel\INFInst
                
                If this flag is used without the '-A' 
                option, only README.TXT will be copied to 
                <Installation Path>.  The directory name can 
                include spaces.  In this case, however, a 
                pair of double quotes (") must enclose the 
                directory name.  This parameter works in 
                either Silent mode or Interactive mode.

-S              Runs the Installer in silent mode.  No user 
                interface is displayed. This flag and the
                '-L' flag must be placed at the end of the 
                command line flag list.
                
Below are the language codes used with the '-L' flag:

    Language                   <LangCode>
    --------                   ----------
    Chinese (PRC)                 0804
    Chinese (Taiwan)              0404
    Danish                        0006
    Dutch                         0013
    English (US)                  0009
    Finnish                       000B
    French (Canadian)             0C0C
    French (Standard)             040C
    German                        0007
    Italian                       0010
    Japanese                      0011
    Korean                        0012
    Norwegian                     0014
    Polish                        0015
    Portuguese (Brazilian)        0416
    Portuguese (Standard)         0816
    Russian                       0019
    Spanish                       000A
    Swedish                       001D
    Thai                          001E


************************************************************
* 5.  CONTENTS OF THE EXTRACTED FILES
************************************************************
INF files are copied to the hard disk drive after running 
the Intel(R) Chipset Software Installation Utility 
executable with a '-A' flag (i.e., "INFINST_ENU.EXE -A -A" 
or "SETUP.EXE -A").  The location of the INF files depends
on whether a '-P' flag is specified along with the '-A' 
flag:

1.  If a '-P' flag is NOT specified, then the INF files are 
    copied to the following directory:  
       "C:\Program Files\Intel\INFINST"
2.  If a '-P' flag IS specified, then the INF files are 
    copied to the location listed immediately after the 
    '-P' flag.  

    See section 4 for more information on flag usage.

After INF file extraction, the INF files and components are 
copied to the <INF Extract Directory>.  These files and 
components are categorized according to the Intel(R) 
Chipset types. The following table summarizes the locations
of the INF files, by chipsets:

   NOTE: The INF files are designed to update ONLY devices
         not supported by the corresponding operating 
         systems.

   NOTE: "<INF Extract Directory>" is abbreviated "<IED>"
         in the remainder of this section.

For each subdirectory of <IED> (e.g., 440MX, ICH, ICH2, or 
PIIXX), the INF files are further classified according to 
the operating systems they are designed for:

   Win95Old\  --->  Contains INF files designed for the
                     Original Release and OSR1 versions 
                     of Windows* 95 ONLY.
   Win95Cur\  --->  Contains INF files designed for the
                     OSR2 and later versions of
                     Windows* 95 ONLY.
   Win98\     --->  Contains INF files designed for
                     Windows* 98 ONLY.
   Win98SE\   --->  Contains INF files designed for
                     Windows* 98 Second Edition ONLY.
   Win2000\   --->  Contains INF files designed for
                     Windows* 2000 ONLY.
   WinME\     ---> Contains INF files designed for
                     Windows* Me ONLY.
   WinXP\     --->  Contains INF files designed for
                     Windows* XP ONLY.


NOTES:
1.  Files in <IED>\440MX\ directory are designed for 
    Intel(R) 440MX Chipset platforms.
2.  Files in <IED>\ICH\ directory are designed for 
    Intel(R) 810, Intel(R) 810E, Intel(R) 820, 
    Intel(R) 840, and Intel(R) 815 Chipset platforms.
3.  Files in <IED>\ICH2\ directory are designed for 
    Intel(R) Chipset platforms with Intel(R) 82801BA
    components.
4.  Files in <IED>\ICH2M\ directory are designed for 
    Intel(R) Chipset platforms with Intel(R) 
    82801BAM components.
5.  Files in <IED>\ICH3M\ directory are designed for 
    Intel(R) Chipset platforms with Intel(R) 82801CAM
    components.								 
6.  Files in <IED>\PIIXX\ directory are designed for 
    Intel(R) 430TX PCIset, Intel(R) 440BX, Intel(R) 440DX,
    Intel(R) 440EX, Intel(R) 440GX, Intel(R) 440LX,
    and Intel(R) 440ZX AGPset platforms.
7.  INFPrelo.INF makes a CUSTOM.INF template that installs 
    the INF files for Intel(R) Chipsets during OS setup.  
    OEMs can incorporate this file into the SETUP directory 
    for the OEM Preload Kit.
    (Refer to Section 8 for more details.)


************************************************************
* 6.  INSTALLING THE SOFTWARE IN INTERACTIVE MODE
************************************************************
1.  Verify that all system requirements have been met as 
    described in section 2.

2.  Run the InstallShield* installation program:
       Self-extracting .EXE distribution: INFINST_xxx.EXE
       Compressed .ZIP distribution     : SETUP.EXE

3.  You will be prompted to agree to the license agreement.  
    If you do not agree, the Installer will exit before 
    extracting any files.
    
4.  Follow the on-screen instructions and use the default
    settings to complete the setup, once the operating
    system has rebooted.

5.  This completes the installation of the Intel(R) Chipset 
    Software Installation Utility.  


************************************************************
* 7.  INSTALLING THE SOFTWARE IN SILENT MODE
************************************************************
1.  Verify that all system requirements have been met as 
    described in section 2.

2.  Run the InstallShield installation program:
    For silent install with auto-reboot:
       Self-extracting .EXE distribution: 
       INFINST_xxx.EXE -a -b -s
       Compressed .ZIP distribution:
       SETUP.EXE -b -s
    - OR -
    For silent install without auto-reboot:
       Self-extracting .EXE distribution: 
       INFINST_xxx.EXE -a -s
       Compressed .ZIP distribution: SETUP.EXE -s

3.  The utility will perform the necessary updates and 
    record the installation status in the following system 
    registry key:
        HKEY_LOCAL_MACHINE\Software\Intel\INFInst

4.  If the utility was invoked with the "-b" flag, the 
    system will automatically reboot if the update was
    successful.

    NOTE:  The system MUST be rebooted for all device 
    Updates to take effect.

5.  To determine whether the install was successful, verify 
    the 'install' value in the registry key specified in 
    Step 3.

    The following table describes the various parameter 
    values:

    Value      Type      Data        Description
    ------     ----      ----        -----------
    "install"  String    "success"   The installation was 
                                     successful.
                         "fail"      The installation was 
                                     not successful.
                                     No INF files were 
                                     copied to the system.                

    "reboot"   String    "Yes"       A reboot is required to 
                                     complete the  
                                     installation.
                         "No"        No reboot is required 
                                     to complete the 
                                     installation.
                                
    "version"  String    <varies>    Current version number 
                                     of the Intel(R) Chipset 
                                     Software Installation 
                                     Utility


************************************************************
* 8.  INSTALLING THE INF FILES PRIOR TO OS INSTALLATION
************************************************************
1.  Copy the OS installation files from the setup 
    directory to a directory on the hard disk.  This 
    procedure requires a large amount of disk space. It 
    is important to make sure there is enough disk space 
    before beginning the copy process.  The directories 
    shall be referred to as follows:

      Windows 2000  :  <WIN2000 Setup Directory>
      Windows 98    :  <WIN98 Setup Directory>
      Windows 98 SE :  <WIN98SE Setup Directory>
      Windows Me    :  <WINMe Setup Directory>
      Windows 95    :  <WIN95 Setup Directory>
  

************************************************************
* 8A.  INSTALLING THE WINDOWS* 2000 INF FILES PRIOR TO
*      OS INSTALLATION
************************************************************
NOTE: The Windows* 2000 OEM Preload Kit distribution CD
      contains a setup directory with all the base OS setup
      files and installation programs (WINNT.EXE and
      WINNT32.EXE).  

The name of the directory may vary depending on the 
distribution CD (e.g., \I386\).


1.  Create the following directory structure under the 
    <WIN2000 Setup Directory>: 

       \$OEM$\$$\INF

2.  Copy the Windows* 2000 INF files from 
    <INF Extract Directory>\XXXX\Win2000 to the directory
    created in Step 1 above:

       <WIN2000 Setup Directory>\$OEM$\$$\INF

    Note: XXXX is the directory name for the chipset of 
          interest.  See Section 8 for more details.

3.  Create the following directory structure under the 
    <WIN2000 Setup Directory>: 

       \$OEM$\$1\drivers\IntelINF

4.  Copy the Windows* 2000 INF files AND the catalog files 
    (.CAT) from <INF Extract Directory>\XXXX\Win2000 to the 
    directory created in Step 4 above:

       <WIN2000 Setup Directory>\$OEM$\$1\drivers\IntelINF

    Note: XXXX is the directory name for the chipset of 
          interest.  See Section 8 for more details.

5.  Either modify the default Windows* 2000 installation
    answer file, UNATTEND.TXT, located in <WIN2000 Setup 
    Directory>, or create a customized answer file.  The
    answer file must include the following information:
   
       [Unattended]
       OemPreinstall = Yes
       OemPnPDriversPath="drivers\IntelINF"

    A sample answer file for preloading the Intel(R) Chipset
    Software Installation utility files is available: 
    <INF Extract Directory>\XXXX\Win2000\INFAnswr.TXT
    
    For more information about Windows* 2000 answer files 
    and unattended installations, please refer to the 
    Microsoft* Windows* 2000 Guide to Unattended Setup.  For
    more information about the \$OEM$ folder, see the 
    Microsoft Windows* 2000 OEM Preinstallation Kit (OPK) 
    User Guide, if you are a computer manufacturer. 
    Otherwise, see the Microsoft Windows* 2000 Deployment 
    Guide.

6.  Run "WINNT.EXE /u:<answer file name> /s:<WIN2000 Setup 
    Directory>" to install Windows* 2000.


************************************************************
* 8B.  INSTALLING THE WINDOWS* 98/Windows* 98 SE/WINDOWS* Me 
*      INF FILES PRIOR TO OS INSTALLATION
************************************************************
NOTE: The Windows* 98, Windows* 98 Second Edition, or  
      Windows* Me OEM Preload Kit distribution CD contains a  
      setup directory with all the base OS setup files 
      (*.CAB) and the installation program (SETUP.EXE).

The name of the directory may vary depending on the 
distribution CD (e.g., \WIN98\).   

1.  Copy the Windows* 98 INF files from the 
    <INF Extract Directory>\XXXX\Win98 to the setup 
    directory identified in Step 1 above, if you are
    preloading Windows* 98.
       -or-
    Copy the Windows* 98 Second Edition INF files from
    <INF Extract Directory>\XXXX\Win98SE to the setup 
    directory identified in Step 1 above, if you are 
    preloading Windows* 98 Second Edition.
       -or-
    Copy the Windows* Me INF files from
    <INF Extract Directory>\XXXX\WinME to the setup 
    directory identified, if you are preloading Windows* Me.  
    
    Note: XXXX is the directory name for the chipset of 
          interest.  See Section 8 for more details.

2.  Depending on your <WIN98 Setup Directory> content,
    there are two cases:

    Case A: CUSTOM.INF file IS NOT present in the 
            <WIN98 Setup Directory>.

            In this case, rename INFPRELO.INF to CUSTOM.INF.

    Case B: CUSTOM.INF file IS present in the 
            <WIN98 Setup Directory>.

            In this case, incorporate the content of 
            INFPRELO.INF into the existing CUSTOM.INF file.  
            For more information, refer to the guidelines 
            for "General Customizations for Preloaded 
            Systems" contained in the Microsoft OEM Preload
            Kit.

3.  Run SETUP.EXE to install Windows* 98.


************************************************************
* 8C.  INSTALLING THE WINDOWS* 95 INF FILES PRIOR TO OS 
*      INSTALLATION
************************************************************
NOTE: The Windows* 95 OEM Preload Kit distribution CD 
      contains a setup directory with all the base OS setup 
      files (*.CAB) and the Windows* 95 installation program 
      (SETUP.EXE).  

The name of the directory may vary depending on the 
distribution CD (e.g., \WIN95\).

NOTE:  The files for Windows* 95 are designed to work solely
       with Windows* 95 (all versions).

1.  If you are installing Windows* 95 Original Release or 
    OSR1, copy the Windows* 95 INF files from <INF Extract 
    Directory>\XXXX\Win95Old to the setup directory 
    identified in Step 1 above, and then proceed to Step 4.
    Otherwise, go to Step 3.

    Note: XXXX is the directory name for the chipset of 
          interest.  See Section 8 for more details.

2.  If you are installing Windows* 95 OSR2 or later, copy  
    the Windows* 95 INF files from <INF Extract 
    Directory>\XXXX\Win95Cur to the setup directory 
    identified in Step 1 above.  

    IMPORTANT:  DO NOT copy the files in the
                <INF Extract Directory>\XXXX\Win95Cur\USB\
                directory to the Step 1 setup directory at 
                this time, even if you intend to install 
                the USB Supplement after the OS setup.

    Note: XXXX is the directory name for the chipset of 
          interest.  See Section 8 for more details.

3.  Depending on your <WIN95 Setup Directory> content, 
    there are two cases:

    Case A: CUSTOM.INF file IS NOT present in the 
            <WIN95 Setup Directory>.

            In this case, rename INFPRELO.INF to 
            CUSTOM.INF.

    Case B: CUSTOM.INF file IS present in the 
            <WIN95 Setup Directory>.

            In this case, incorporate the content of 
            INFPRELO.INF into the existing CUSTOM.INF file.  
            For more information, refer to the guidelines 
            for "General Customizations for Preloaded 
            Systems" contained in the Microsoft OEM Preload
            Kit.

4.  Run SETUP.EXE to install Windows* 95.

    If you are installing Windows* 95 Original Release, OSR1 
    or OSR2 without the USB Supplement, the installation is 
    complete.

    Steps 5 and after are needed only if Windows* 95 OSR2 or 
    a subsequent version is being installed, AND if you 
    intend to install the USB Supplement.  Refer to the 
    System Requirements section for more information.

5.  Run Device Manager to prepare for the update of the
    USB device driver:

    a.  Click on Start.
    b.  Select Settings.
    c.  Select Control Panel.
    d.  Double-click on System icon.
    e.  Click on Device Manager tab.
    f.  Click on View Devices by Connection button.
    g.  Click on Plug and Play BIOS.
    h.  Click on PCI.
    i.  Click on PCI Universal Serial Bus.
    j.  Click on Remove.

6.  If you are updating an Intel(R) 82440MX Chipset 
    platform, copy 440MXUSB.INF from the
    <INF Extract Directory>\440MX\Win95Cur\USB directory to 
    the <WINDOWS Directory>\INF directory, and then proceed
    to Step 11. Otherwise, go to Step 8.

7.  If you are updating an Intel(R) 810, Intel(R) 820 or
    Intel(R) 840 Chipset platform, copy ICHxUSB.INF from 
    the <INF Extract Directory>\ICH\Win95Cur\USB directory 
    to the <WINDOWS Directory>\INF directory, and then 
    proceed to Step 11. Otherwise, go to Step 9.

8.  If you are updating an Intel(R) Chipset platform with 
    "ICH2" components, copy ICH2USB.INF from the
    <INF Extract Directory>\ICH2\Win95Cur\USB directory to 
    the <WINDOWS Directory>\INF directory, and then proceed
    to Step 11. Otherwise, go to Step 10.

9.  If you are updating an Intel(R) Chipset platform with 
    PIIX3 or PIIX4 components, copy PIIXXUSB.INF from the
    <INF Extract Directory>\PIIXX\Win95Cur\USB directory to 
    the <WINDOWS Directory>\INF directory.

10. Install the Windows* 95 "USB Supplement" executable.
    Follow screen prompts to reboot the system.

This completes the setup.


************************************************************
* 9.  INSTALLING THE INF FILES AFTER OS INSTALLATION
************************************************************
************************************************************
* 9A.  INSTALLING THE WINDOWS* 2000 INF FILES AFTER OS 
*      INSTALLATION
************************************************************
Some Intel chipset platforms already are supported by 
Windows* 2000, so it may not be necessary to use the INF 
files provided by this software to update Windows* 2000.

The following steps describe the installation process of
the Windows* 2000 INF files.  You may need to repeat these 
steps to update all Intel chipset devices not supported
by Windows* 2000.

    1.  Copy the contents of the 
        <INF Extract Directory>\XXXX\Win2000 
        directory to the root directory of the floppy disk
        (A:\).
        
        Note: XXXX is the directory name for the chipset 
              of interest.
              See Section 8 for more details.
    2.  Close all programs currently running on the system.
    3.  Click on Start.
    4.  Select Settings.
    5.  Select Control Panel.
    6.  Double-click on System icon.
    7.  Click on Hardware tab.
    8.  Click on Device Manager button.
    9.  Select "Devices by connection" under the View menu.
    10. Click on MPS Uniprocessor PC -OR- MPS 
        Multiprocessor PC.
        NOTE:  Only one of the above items will be 
               displayed for a given system.
    11. Click on PCI bus.
    12. Right-click on the line containing the description
            PCI standard host CPU bridge
            -or-
            PCI standard ISA bridge
            -or-
            PCI standard PCI-to-PCI bridge
            -or- 
            PCI System Management Bus
            -or- 
            Standard Dual PCI IDE Controller
            -or-
            Standard Universal PCI to USB Host Controller
            (This line will be selected.)
    13. Select Properties from the pull-down menu.
    14. Click on the Driver tab.
    15. Click on Update Driver button.
    16. Windows* 2000 will launch the Upgrade Device Driver 
        Wizard.  Select Next.
    17. Ensure that the following choice is selected:
            Search for a suitable driver for my device 
            (recommended)
    18. Insert the floppy containing the Windows* 2000 INF 
        files into the floppy drive.
    19. Select Next.
    20. Windows* 2000 will list locations from where the 
        updated driver file can be found.  Ensure that the 
        following choice is selected:
            Floppy disk drives
    21. Select Next.
    22. Windows* 2000 should report that a driver has been
        found:
            (The detected device name will be displayed.)
        Select Next.            
    23. Select Finish.
    24. Restart the system when prompted to do so.


************************************************************
* 9B.  INSTALLING THE WINDOWS* 98/Windows* 98 SE/WINDOWS* 
*      Me/WINDOWS* 95 INF FILES AFTER OS INSTALLATION
************************************************************
Some Intel chipset platforms already are supported by 
Windows* 98 Second Edition and Windows* Me, so it may not be 
necessary to use the INF files provided by this software to 
update these operating systems.

The following steps describe the installation process for
the Windows* 98, Windows* 98 Second Edition, Windows* Me and 
Windows* 95 INF files.  You may need to repeat these steps 
to update all Intel chipset devices not supported by these 
operating systems.

    1.  Depending on the operating system you intend to 
        update, copy the contents of one of the following 
        directories to the root directory of the floppy 
        disk (A:\).

        For Windows* 98: 
                 <INF Extract Directory>\XXXX\Win98
        For Windows* 98 Second Edition: 
                 <INF Extract Directory>\XXXX\Win98SE
        For Windows* Me: 
                 <INF Extract Directory>\XXXX\WinME
        For Windows* 95 Retail or OSR1:
                 <INF Extract Directory>\XXXX\Win95Old
        For Windows* 95 OSR2 or later:
                 <INF Extract Directory>\XXXX\Win95Cur

        Note: XXXX is the directory name for the chipset of
              interest.
              See Section 8 for more details.
    2.  Close all programs currently running on the system.
    3.  Click on Start.
    4.  Select Settings.
    5.  Select Control Panel.
    6.  Double click on System icon.
    7.  Click on Device Manager tab.
    8.  Click on View Devices by Connection button.
    9.  Click on Plug and Play BIOS, or Advanced Configuration
        and Power Interface (ACPI) BIOS.
        NOTE:  Only one of the above items will be 
               displayed for a given system.
    10. Click on PCI bus.
    11. Click on the line containing the description
            PCI standard host CPU bridge
            -or-
            PCI standard ISA bridge
            -or-
            PCI standard PCI-to-PCI bridge
            -or- 
            PCI System Management Bus
            -or- 
            Standard Dual PCI IDE Controller
            -or-
            Standard Universal PCI to USB Host Controller
            (This line will be selected.)
    12. Click on the Remove button at the bottom of the 
        window.
    13. If more than one Intel chipset device needs 
        updating, go to Step 11 to remove more devices.
    14. When prompted to restart the system, select Yes.
    15. Restart the system.
    16. The Windows operating system will launch the Add
        New Hardware Wizard.
        Select Next in the dialog box that states:
            "This wizard searches for new drivers for:"
    17. Ensure that the following choice is selected:
            Search for the best driver for your device 
            (Recommended)
    18. Select Next.
    19. Insert the floppy containing the .INF files into
        the floppy drive.
    20. Ensure that the following choice is selected:
            Floppy disk drives
    21. If the .INF files are not located in the root 
        directory of the floppy disk, also select the 
        following and enter the path to the .INF files
        needed to update this operating system:
            Specify a location:
    22. Select Next.
    23. The Windows operating system should report that
        the driver has been found and that it is "now 
        ready to install the best driver for this 
        device."
    24. Select Next.
    25. Select Finish.
    26. The Windows operating system may prompt you to 
        install additional drivers if more than one device
        was removed during Steps 11 through 13. Follow the 
        same procedure to install the remaining Intel 
        chipset devices.
    27. Restart the system when prompted to do so.


************************************************************
* 10.  VERIFYING INSTALLATION OF THE SOFTWARE
************************************************************
Run Device Manager to verify the correct installation and
usage of the INF files.

For Windows* 95, Windows* 98 and Windows* 98 Second Edition 
and Windows* Me:

   1.  Click on Start.
   2.  Select Settings.
   3.  Select Control Panel.
   4.  Double-click on System icon.
   5.  Click on Device Manager tab.
   6.  Click on View Devices by Connection button.
   7.  Click on Plug and Play BIOS, or Advanced 
       Configuration and Power Interface (ACPI) BIOS.
   8.  Click on PCI bus.

For Windows* 2000:

   1.  Click on Start.
   2.  Select Settings.
   3.  Select Control Panel.
   4.  Double-click on System icon.
   5.  Click on Hardware tab.
   6.  Click on Device Manager button.
   7.  From the View menu, select menu item Devices by 
       connection.
   8.  Click on Standard PC, or Advanced Configuration and 
       Power Interface (ACPI) PC.
   9.  Click on Microsoft ACPI Compliant System
  10.  Click on PCI bus.

After the Device Manager is launched as described above, 
check the descriptions for the following entries:

    *** NOTE:  Device Manager will display only the names of 
               devices currently detected in the system.

    Intel(R) 810 Chipset:
        Intel(R) 82810 System and Graphics Controller 
        -or-
        Intel(R) 82810 DC-100 System and Graphics 
           Controller
  
    Intel(R) 810E Chipset, Intel(R) 810E2 Chipset:
        Intel(R) 82810E DC-133 System and Graphics 
           Controller 

    Intel(R) 820 Chipset, Intel(R) 820E Chipset:
        Intel(R) 82820 Processor to I/O Controller
        Intel(R) 82820 Processor to AGP Controller

    Intel(R) 840 Chipset:
        Intel(R) 82840 Processor to I/O Controller 
        Intel(R) 82840 Processor to AGP Controller 
        Intel(R) 82840 PCI Bridge 
              
     Intel(R) 82806AA PCI 64-bit Hub:
        Intel(R) 82806AA Advanced Programmable Interrupt 
        Controller
        Intel(R) 82806AA PCI Bridge
        Intel(R) 82806AA Controller (reserved)

    Intel(R) 82801AA I/O Controller Hub (ICH):
        Intel(R) 82801AA LPC Interface Controller 
        Intel(R) 82801AA Ultra ATA Controller 
        Intel(R) 82801AA USB Universal Host Controller 
        Intel(R) 82801AA SMBus Controller 
        Intel(R) 82801AA PCI Bridge 
      
    Intel(R) 82801AB I/O Controller Hub (ICH0):
        Intel(R) 82801AB LPC Interface Controller 
        Intel(R) 82801AB Ultra ATA Controller 
        Intel(R) 82801AB USB Universal Host Controller 
        Intel(R) 82801AB SMBus Controller 
        Intel(R) 82801AB PCI Bridge 

    Intel(R) 82371AB PCI to ISA/IDE Xcelerator (PIIX4):
        Intel(R) 82371AB PCI to ISA bridge (EIO mode)
        Intel(R) 82371AB PCI to ISA bridge (ISA mode)
        Intel(R) 82371AB Power Management Controller
        Intel(R) 82371AB/EB/MB PCI Bus Master IDE 
           Controller
        Intel(R) 82371AB/EB/MB PCI to USB Universal Host
           Controller
   
    Intel(R) 82371EB/MB PCI to ISA/IDE Xcelerator (PIIX4):
        Intel(R) 82371EB/MB PCI to ISA bridge (EIO mode)
        Intel(R) 82371EB/MB PCI to ISA bridge (ISA mode)
        Intel(R) 82371EB/MB Power Management Controller
        Intel(R) 82371AB/EB/MB PCI Bus Master IDE 
           Controller
        Intel(R) 82371AB/EB/MB PCI to USB Universal Host
           Controller

    Intel(R) 82371SB PCI to ISA/IDE Xcelerator (PIIX3):
        Intel(R) 82371SB PCI to ISA bridge
        Intel(R) 82371SB PCI Bus Master IDE Controller
        Intel(R) 82371SB PCI to USB Universal Host 
           Controller    

    Intel(R) 440MX Chipset:
        Intel(R) 82440MX Processor to I/O Controller
        Intel(R) 82440MX PCI to ISA Bridge
        Intel(R) 82440MX Power Management Controller
        Intel(R) 82440MX Bus Master IDE Controller
        Intel(R) 82440MX USB Universal Host Controller

    Intel(R) 430TX PCIset:
        Intel(R) 82443TX Processor to PCI bridge

    Intel(R) 440BX AGPset, Intel(R) 440DX AGPset, 
      Intel(R) 440ZX AGPset:
        Intel(R) 82443BX/ZX/DX Processor to PCI bridge
        Intel(R) 82443BX/ZX/DX Processor to AGP controller

    Intel(R) 440GX AGPset:
        Intel(R) 82443GX Processor to PCI bridge
        Intel(R) 82443GX Processor to AGP controller

    Intel(R) 440LX AGPset:
        Intel(R) 82443LX Processor to PCI bridge
        Intel(R) 82443LX Processor to AGP controller

    Intel(R) 815 Chipset, Intel(R) 815E Chipset, Intel(R) 
    815EP Chipset, Intel(R) 815EM Chipset:
        Intel(R) 82815 Processor to I/O Controller - 1130 
        Intel(R) 82815 Processor to AGP Controller - 1131 

    Intel(R) 82801BA I/O Controller Hub:
        Intel(R) 82801BA LPC Interface Controller - 2440 
        Intel(R) 82801BA PCI Bridge - 244E 
        Intel(R) 82801BA Ultra ATA Storage Controller - 244B 
        Intel(R) 82801BA/BAM SMBus Controller - 2443 
        Intel(R) 82801BA/BAM USB Universal Host  Controller 
                 - 2442 
        Intel(R) 82801BA/BAM USB Universal Host Controller 
                 - 2444 
        Intel(R) 82801BA/BAM AC '97 Audio Controller - 2445 

    Intel(R) 82801BAM I/O Controller Hub:
        Intel(R) 82801BAM LPC Interface Controller - 244C 
        Intel(R) 82801BAM PCI Bridge - 2448 
        Intel(R) 82801BAM Ultra ATA Storage Controller 
                 - 244A
        Intel(R) 82801BA/BAM SMBus Controller - 2443 
        Intel(R) 82801BA/BAM USB Universal Host Controller 
                 - 2442 
        Intel(R) 82801BA/BAM USB Universal Host Controller 
                 - 2444 
        Intel(R) 82801BA/BAM AC '97 Audio Controller - 2445 

    Intel(R) 850 Chipset:
        Intel(R) 82850 Processor to I/O Controller - 2530 
        Intel(R) 82850/82860 Processor to AGP Controller 
                - 2532       

   Intel(R) 860 Chipset:
       Intel(R) 82860 Processor to I/O Controller - 2531
       Intel(R) 82850/82860 Processor to AGP Controller 
                - 2532 
       Intel(R) 82860 PCI Bridge - 2533
       Intel(R) 82860 Controller (reserved) - 2537      

   Intel(R) 830M Chipset:
       Intel(R) 82830 Processor to I/O Controller - 3575 
       Intel(R) 82830 Processor to AGP Controller - 3576 
       Intel(R) 82830 Processor to I/O Controller - 3578 

   Intel(R) 82801CAM I/O Controller Hub:
        Intel(R) 82801CAM PCI Bridge - 2448
        Intel(R) 82801CAM LPC Interface Controller - 248C 
        Intel(R) 82801CAM Ultra ATA Storage Controller 
                 - 248A 
        Intel(R) 82801CA/CAM SMBus Controller - 2483 
        Intel(R) 82801CA/CAM USB Universal Host Controller 
                 - 2482 
        Intel(R) 82801CA/CAM USB Universal Host Controller 
                 - 2484 
        Intel(R) 82801CA/CAM USB Universal Host Controller 
                 - 2487 
        Intel(R) 82801CA/CAM AC '97 Audio Controller - 2485

   
   Intel(R) 845 Chipset
        Intel(R) 82845 Processor to I/O Controller - 1A30
        Intel(R) 82845 Processor to AGP Controller - 1A31


11. On certain systems, the following device may also be 
    updated:
 
     a. Click on View Devices by Connection button.
     b. Click on Plug & Play BIOS, or Advanced Configuration 
        and Power Interface (ACPI) BIOS.     
     c. Verify that the following entry is present:
        Intel(R) 82802 Firmware Hub Device -OR-
        Intel(R) Security Driver


************************************************************
* 11.  IDENTIFYING THE SOFTWARE VERSION NUMBER
************************************************************
The version of the software included in the distribution
package is specified in the file RELNOTES.HTM.  

The version of the software included in the distribution 
package can also be identified by examining the following 
registry location:

    Key name:   \\HKEY_LOCAL_MACHINE\Software\Intel\InfInst
    Value name: version


************************************************************
* 12.  TROUBLESHOOTING
************************************************************
It is assumed that the system requirements in Section 2 
above have been satisfied.

Issue:      System locks up during Device Manager Remove or 
            during restart.

Solution:   System lockup can occur during Restart as a 
            result of several possible system issues.  In 
            the event of system lockup, restart the machine 
            and view Device Manager.  If devices are listed 
            properly and the system experiences no further 
            problems, then the .INF file restore process was 
            successful.  If devices are not configured 
            correctly, try re-running the procedures 
            outlined in Section 3.

            If this does not fix problems or further 
            problems are experienced, reinstall the 
            operating system.


Issue:      After running the setup program and rebooting 
            the machine, Windows reports that it cannot find 
            one of the following files:
                  ESDI_506.pdr

Solution:   Click Browse in the dialog box where this 
            problem occurs, locate the

                  <Windows>\System\IOSubsys

            directory and click OK. The system should
            be able to locate this file in this directory 
            and continue re-enumerating for the new devices.

Issue:      After running the setup program and rebooting 
            the machine, Windows reports that it cannot find 
            one of the following files:
 
                  UHCD.SYS
                  USBD.SYS
                  USBHUB.SYS

Solution:   Click Browse in the dialog box where this 
            problem occurs, locate the

                  <Windows>\System32\drivers 
                  (for Windows* 98, Windows* Me)
                   -or-
                  <Windows>\System (for Windows* 95)

            directory, and click OK.  The system should
            be able to locate this file in this directory 
            and continue re-enumerating for the new devices.

Issue:      During setup, installation stops and prompts for 
            one of the following files:
      
                  UHCD.SYS
                  USBD.SYS
                  USBHUB.SYS

Solution:   Ensure that the Windows* 95 USB Supplement has 
            been installed prior to running the Intel(R)  
            Chipset Software Installation Utility setup  
            program.

Issue:      After running the setup program and rebooting 
            the machine, Windows reports that it cannot find 
            the following file:
                  isapnp.vxd

Solution:   Click Browse in the dialog box where this 
            problem occurs, locate the

                  <Windows>\System

            directory, and click OK.  The system should
            be able to locate this file in this directory 
            and continue re-enumerating for the new devices.

Issue:      After performing the silent install, the 
            HKLM\Software\Intel\InfInst key was not created 
            or the data of the value "install" is not 
            "success".

Solution:   This is caused by one of the following 
            scenarios:
               - The current system does not contain 
                 a supported operating system, or
               - The current system does not contain 
                 a supported chipset.

            Verify the System Requirements in Section 2.


************************************************************
* DISCLAIMER
************************************************************
Intel is making no claims of usability, efficacy or 
warranty.  
The INTEL SOFTWARE LICENSE AGREEMENT
(OEM / IHV / ISV Distribution & Single User) 
completely defines the licensed use of this software.
************************************************************
Information in this document is provided in connection with 
Intel products.  No license, express or implied, by estoppel 
or otherwise, to any intellectual property rights is granted 
by this document.  Intel assumes no liability whatsoever, 
and Intel disclaims any express or implied warranty 
relating to sale and/or use of Intel products, including 
liability or warranties relating to fitness for a particular 
purpose, merchantability or infringement of any patent, 
copyright or other intellectual property right.  Intel 
products are not intended for use in medical, life saving, 
or life-sustaining applications.

************************************************************
Intel Corporation disclaims all warranties and liabilities 
for the use of this document and the information contained 
herein, and assumes no responsibility for any errors which 
may appear in this document, nor does Intel make a 
commitment to update the information contained herein.  
Intel reserves the right to make changes to this document at 
any time, without notice.
************************************************************
************************************************************

* Third-party brands and names are the property of their 
respective owners.

Copyright (c) Intel Corporation, 1997-2001




