HEIDI.TXT

Version 1.61

To install the latest version of your 3Dlabs Heidi driver, locate
your 3DStudio Max 1.x directory on your hard drive and then enter
the Drivers sub-directory. Rename the file in there 'wglint.hdi'
to 'wglint.bak'. Then copy the new 'wglint.hdi' from this floppy,
to the Drivers directory.

You can now run 3DStudio Max, and the new driver will be used.

Please note that when using the 3Dlabs Heidi driver under Windows 95 
the following software components must also be installed:

	Direct X version 3 or later, and
	The Microsoft OpenGL binaries, opengl32.dll and glu32.dll.

If using Permedia cards, the best performance can be achieved
through running in 32768 color mode.

If using GLINT cards, the best performance can be achieved by
running in TrueColor.

GLINT GMX boards should be used with OpenGL acceleration
under 3D Studio MAX 2. Although 3D Studio MAX 1.x will run you will
not obtain full acceleration with a Heidi driver.