Release Version:2.20

[INSTALLING THE AUDIORACK32]

You must have Windows 95 or Windows NT installed prior to using the 
AudioRack32. After placing the AudioRack32 disk in a floppy drive, 
click START on the taskbar and choose RUN from the popup menu.

In the Run dialog box, type the letter of the drive and "setup" (for
example, a:\setup), then click OK.

The first AudioRack32 Setup dialog box appears. Note the instructions,
then click NEXT to proceed or CANCEL to leave Setup.

Next the Choose Destination Location dialog box appears. Click NEXT to
install the AudioRack32 in the default directory or BROWSE to choose a
different directory. When you are done click OK or CANCEL to return to 
the Choose Destination Location dialog box.

If the directory you designate doesn't exist, you will be asked to 
confirm your selection. Click YES to proceed or NO to go back and enter
a new destination directory. 

Once you have chosen the default directory or entered a directory of 
your own choosing, the Setup program will install the AudioRack32.


[NEW FEATURES]

>> USE AUDIORACK CD PLAYER AS THE DEFAULT CD PLAYER
During installation, you will be asked if you want to use AudioRack
CD player as the default CD player.  Normally Windows 95 CD player is
the default.  If you answer "YES", the installation program will
overwrite the value of the key [HKEY_CLASSES_ROOT]\AudioCD\shell\play\command
in registry.  You may switch back to Windows 95 CD player any time by 
resetting this key value.


>> PLAYBACK MIXER AND RECORD MIXER DISPLAY
The MixerRak provides the added feature of displaying the mixer channel inputs
that are not shown on the MixerRak.  The MixerRak can only display six inputs
at one time.
Clicking either handle bar of the MixerRak will scroll the input channels
to the left or to the right, thus showing the "hidden channels", provided
the AudioDrive device supports more than six mixer inputs.


[LIMITATIONS]

>> RECORD MODE AND THE ES1868
If your audio hardware includes the ES1868 AudioDrive chip, the Monitor 
button and Master Volume controls will be disabled in Record Mode. The 
ES1868 does not support these functions in Record Mode. For more 
information see "Multiplexers" in the Online Help or the AudioRack32 for 
Windows95 User Guide.


[TECHNICAL SUPPORT]

Please contact your hardware manufacturer/vendor for upgrades and 
technical support.

07/09/98