Intel(r) Ultra ATA Storage Driver Setup
README.TXT

Description
===========
The Intel Ultra ATA Storage Driver automatically enables fast Ultra ATA transfers for a variety of ATA/ATAPI mass storage devices such as hard disk drives and CD-ROMs.  This driver has been architected to take advantage of the latest Intel Ultra ATA controller features to improve both storage subsystem performance and overall system performance.  Driver installation is fully automated for Microsoft* Windows* 98, Microsoft* Windows* NT* 4.0, and Microsoft* Windows* 2000.

System Requirements
===================
Microsoft Windows 98, Microsoft Windows NT 4.0 or Microsoft Windows 2000 (any Service Pack)
Intel 80801AA, 82801AB, or 82801BA controllers

Basic Installation Instructions
===============================
- Run SETUP.EXE and answer all prompts
- You will be prompted to reboot when installation is complete

Note:  By default, all general files (README.TXT, etc.) are copied to the
       path <bootdrive>:\Program Files\Intel\Ultra ATA Storage Driver

Verifying Correct Installation
==============================
Microsoft Windows 98:  
  - Run 'Start', 'Settings', then 'ControlPanel'
  - Double-click 'System' Control Panel Application
  - Select the 'Device Manager' tab
  - Expand the 'Hard Disk Controllers' entry
  - Select either the 'Primary' or 'Secondary' controller listed
  - Select the 'Properties' button
  - Select the 'Driver' tab
  - Select the 'Driver File Details' button
  - 'INTELATA.MPD' and 'INTELVSD.VXD' should be displayed

Microsoft Windows NT 4.0:
  - Run Start/Settings/ControlPanel
  - Double-click SCSI Adapters
  - Select the Devices tab
  - 'IntelATA' or 'Intel Ultra ATA Controller' should be displayed
  
Microsoft Windows 2000:  
  - Run 'Start', 'Settings', then 'ControlPanel'
  - Double-click 'System' Control Panel Application
  - Select the 'Hardware' tab
  - Select 'Device Manager' button
  - Expand the 'IDE ATA/ATAPI Controllers' entry
  - Select the 'Intel 82801XX Ultra ATA Controller' listed,
    where XX in 82801XX represents the controller identified by the 
    'System Requirements' section of this document. 
  - Select the 'Properties' button
  - Select the 'Driver' tab
  - Select the 'Driver File Details' button
  - 'INTELATA.SYS' should be displayed


Advanced Installation Instructions
==================================
The following  SETUP flags are available:
  -?           Help information for the setup flags (shown below)
  -S           Silent install (no user prompts)
  -B           Forces a system reboot after installation
  -P <path>    Supplies target installation path
  -A           Extracts all driver files (does not install driver) to <path>
               if -P is also supplied, or the default directory otherwise
  -N           Installs all components except driver
  -O <name>    Supplies target Start Menu Program Folder name if installing
               Companion applet
  -L<number>   Forces a particular language install (See the product
               documentation for a table mapping <number> to language)
  -build       Displays build number
  -back        Sets up a full windowed installer
  -nocompanion Prevents the installation of the Companion application

Notes:  Flags and their parameters are not case-sensitive.  
        Flags may be supplied in any order, with the exception of the -S and
        -L flags which must be supplied last.
        When using the -A flag, a target path may be specified via the -P
        flag, and the -O, -L, -S, and -N flags are ignored.
        When using the -P or -O flags, a space is required between the flag
        and the argument; when using -L, however, there should be no space.

To load the driver via the method outlined in the Microsoft document, "Deployment Guide Automating Windows NT Setup," use the supplied TXTSETUP.OEM file included in this driver package and insert the lines below into the UNATTEND.TXT file.  This method is available for both Microsoft Windows NT 4.0 and Microsoft Windows 2000. (The TXTSETUP.OEM, INTELATA.INF, and INTELATA.SYS file need to first be extracted from the compressed .CAB file. To extract these files, run 'SETUP -A -P <path>' as described above.)

Microsoft Windows NT 4.0:
  // Insert the lines below into the UNATTEND.TXT file
   [MassStorageDrivers]
  "Intel Ultra ATA Controller" = OEM

  [OEMBootFiles]
  INTELATA.INF
  INTELATA.SYS
  TXTSETUP.OEM

Microsoft Windows 2000:
  // Insert the lines below into the UNATTEND.TXT file
  [MassStorageDrivers]
 "Intel Ultra ATA Controller" = OEM

  [OEMBootFiles]
  INTELATA.INF
  INTELATA.SYS
  TXTSETUP.OEM



Removing the Software
=====================
- Run Start/Settings/ControlPanel
- Select the Add/Remove button
- Select the "Intel Ultra ATA Storage Driver" for removal
- Click on Yes when the script prompts for confirmation
- The uninstall script will prompt you to restart the system

Support Information
===================
Contact your system provider, or visit http://support.intel.com for the
latest troubleshooting information.

==========
DISCLAIMER
==========
Intel is making no claims of usability, efficacy or warranty.  
The INTEL SOFTWARE LICENSE AGREEMENT
(OEM / ISV Distribution & Single User) 
completely defines the licensed use of this software.
************************************************************
Information in this document is provided in connection with 
Intel products.  No license, express or implied, by estoppel 
or otherwise, to any intellectual property rights is granted 
by this document.  Intel assumes no liability whatsoever, 
and Intel disclaims any express or implied warranty 
relating to sale and/or use of Intel products, including 
liability or warranties relating to fitness for a particular 
purpose, merchantability or infringement of any patent, 
copyright or other intellectual property right.  Intel 
products are not intended for use in medical, life saving, 
or life-sustaining applications.

************************************************************
Intel Corporation disclaims all warranties and liabilities 
for the use of this document and the information contained 
herein, and assumes no responsibility for any errors which 
may appear in this document, nor does Intel make a 
commitment to update the information contained herein.  Intel 
reserves the right to make changes to this document at any 
time, without notice.
************************************************************
************************************************************

* Third-party brands and names are the property of their 
respective owners.

Copyright (c) Intel Corporation, 1997-2000
